In this folder you will find:

* ZIPPED File ( Cleveland\_UI\_V1\_1\_2 ). Copy this to a USB drive as is. DO NOT unzip folder.
* Video showing process to update ( usb\_update ). This will require that you have the USB attached to UI with the zipped file above.
* The USB connection to use is shown in the attached picture ( USB Connector ). Important you should see 2 USB connectors most likely with a cap installed. One connector line has a black tape around it and SHOULD NOT be used. (See picture)  
  The other connect does NOT have any tape, this one you can remove the end cap and connect USB stich here. (See picture)

Once you have unit running and USB (with update version 1.1.2 ) connected, Enter Settings mode and select Software Update and you should see new update version listed. Select it and follow the video showing the messages you will see and the required steps to update the UI.

Initially because this UNIT was not configured permission to allow a AUTOMATIC reboot, after some time (video says WAIT 40 – 50 seconds \_\_\_PLEASE WAIT) and then remove power Manually and then reinstall power. Keep following the UI as the system should now begin the actual software update and should reboot automatically this time as now permission has been written into the system and now updates will no longer require USER to manually cycle powe.