Initial UI update attempt from Cleveland\_UI\_V1\_1\_0 to Cleveland\_UI\_V1\_1\_1

Because we didn’t fully understand the update process from a USB at the time version 1.1.0 was released there may be a one-time process required to update the UI to version 1.1.1.

To update the UI the .tgz file must be loaded onto a USB stick. The UI versions can be found on the Cleveland repos in the UI Releases folder. These versions are a compressed (tgz) file and must be copied as-is to the USB stick.

1. Ensure UI update file is on USB stick.
2. Connect the USB stick to the UI extender cable from the UI.
3. On the UI Home screen select the Settings Cam image to enter the current Settings mode. (note once Settings and Service mode are specified this screen will be different.)
4. Select Software Update
5. On screen select the file you want to update.
6. A confirmation screen should be displayed with information concerning update. Confirm update
7. Another screen should report back that update is in progress.  
   DO NOT remove USB stick or turn power Off.
8. Wait for over a minute and IF UI has not rebooted, the following process must be done. (this is caused by version 1.1.0 not allowing permission to reboot UI)
9. Tap on UI screen and the process will now have to be repeated.
10. Select the version on screen to update (Cleveland\_UI\_V1\_1\_1)
11. The confirmation screen again needs to confirmed and the update process will begin as before.
12. After sometime (up to a minute), the UI should reboot automatically indicating the update has been completed.